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EXHIBIT" D * 71620898

66" Brick Column Acme 1776

24" WIDTH

4 "white concretc cast cap (25" Column Cap)

No. § iar of Steel
4 into column

18" footing

1/2" anchor bokts.

6" Cedar Privacy Fence (Dog Ear Type)

Columns to be spaced every 30°

30" deep pler B

10° pler.
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7.14 Fences

Any fences erected by owners of lots abutting collector
streets within the subdivision will be in accordance with. the
materials, description, and measurements shown on Exhibit *D"
hereto.




